1. **Purpose of this Equipment:** To provide employees an all-weather break area away from building.
2. **Federal Supply Class:** 5670
3. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 10 foot Octagonal design. Dimensional sizes, such as length, width, and height are not critical to this equipment except that is serves as a general guide to keep this equipment sized for available space.
   2. **Salient Characteristics that shall be provided:**
      1. Octagonal design.
      2. Waterproof treated wood with rounded edges.
      3. Full screen enclosure.
      4. Mounted benches.
      5. Door with screen.
      6. Asphalt shingle roof.
      7. Gazebo step at the entry point.

# Industry Standards / Requirement(s): N / A

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Natural.

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped assembled.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions:

# Store: Provide a level area for the unit, which is accessible by a slant bed truck for

# unloading. Provide a fork lift and driver to help position this unit as required.

# Contractor: Fully assembled unit shipped on a self-unloading slant bed truck, placed on a store specified location and leveled / braced as required.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****