# Purpose of this Equipment: To safely store propane tanks in centralized area.

1. **Federal Supply Class:** 7125
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 40 inches long / wide, 33 inches deep, 71 inches high.
   2. **Salient Characteristics that shall be provided:**
      1. Cabinet designed to hold eight (8) LP gas cylinders (30 gallon) on their side
      2. Internal shelves for spacing of the cylinders
      3. Lockable wire mesh doors
      4. Side panels constructed of minimum 13 gauge, wire mesh
      5. Top panel constructed of minimum 12 gauge steel
      6. Pre-drilled holes in foot pads for securing unit to floor

# Industry Standards / Requirement(s):

* + 1. **Industry Standards:** Requires compliance with the Occupational Safety and Health Administration (OSHA) standard 1910.106, flammable and combustible liquids, and the National Board of Fire Underwriters flammable and combustible liquid code 30 as recommended by the National Fire Protection Association (NFPA).
    2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Safety yellow with red lettering.

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use***.***
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Commercial Point of Contact for Service.
     2. Installation and Operating Instructions.
     3. Parts List***.***

# Special Coordinating / Safety Instructions:

* 1. **Store**: This cabinet should be placed outside at least 50 feet from the commissary building or as directed by the local installation Fire Department.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

