# Purpose of this Equipment: To provide a protective, laminated finish on letters, legal size documents, certificates and identification cards.

# Federal Supply Class: 7490

1. **General Operating Specifications:**
	1. **Dimensions:**
		1. 19 inches long / wide, 9 inches deep, 4 inches high. Dimensional sizes, such as length, width, and height may vary no more than 3 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Unit to be a stand-by (heat ready) pouch laminator.
		2. Lamination width to be 12 inches.
		3. Able to laminate film up to 10 millimeters in thickness.
		4. 2 sets of pressure rollers (4 each).
		5. On/off switch.
		6. Adjustable temperature control.

# Industry Standards / Requirement(s):

* + 1. Underwriters Laboratory (UL) listed or approved equivalent. CE is not acceptable for a standard.
		2. Energy Star Compliant
		3. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

# Electrical Requirements:

# 120 volts, 60 Hertz, 1 phase, with an average amperage draw of 9 amps.

# 4.2 Minimum 6 foot cord with a NEMA standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements.

#

# Standard Contractor Requirements:

* 1. Must be shipped ready to plug in and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Commercial Warranty and Point of Contact for Warranty Service.
		2. Installation and Operating Instructions.
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****