# Purpose of this Equipment: To heat or cook food items in break rooms and deli.

1. **Federal Supply Class:** 7290
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Minimum 20 inches long / wide, 16 inches deep, 12 inches high.
   2. **Salient Characteristics that shall be provided:**
      1. Minimum 1000 watts.
      2. Minimum 0.8 cubic feet oven capacity.
      3. Lighted interior cavity.
      4. Tempered glass window in door or see-through oven door.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: Underwriters Laboratory (UL) listed and National Sanitation Foundation (NSF) certification, or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# \_\_\_\_\_ Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# Minimum 5 foot cord with a NEMA Standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements.

# NOTE: the operating range for 120 volts is 110 to 120 volts.

# Standard Contractor Requirements:

* 1. Must be shipped ready to plug in and use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****