# Purpose of this Equipment: To provide 360 degree bakery goods, multi-tiered display for patron self-service selections.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Overall height to be approximately 54 inches.
		2. 72 inches long / wide, 30 inches deep, (Base section).
		3. 66 inches long / wide, 28 inches deep, (Second shelf / display level).
		4. 60 inches long / wide, 21 inches deep, (Third shelf / display level).
		5. 54 inches long / wide, 15 inches deep, (Top shelf /display level).
		6. Dimensional sizes may vary plus or minus 2 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Oak construction.
		2. Moisture resistant protective sealant.
		3. Casters: 2 swivel and minimum 2 locking.
		4. Base section to have a black plastic or flexible vinyl bumper on front and back.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****