# Purpose of this Equipment: To provide 360 degree bakery goods, multi-tiered display for patron self-service selections.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Base section:
         1. 45 inches long / wide, 45 inches deep, 45 inches high. (Overall).
         2. 44 inches long / wide, 17 inches deep, (First shelf / display level).
         3. 44 inches long / wide, 14 inches deep, (Second shelf / display level).
         4. 44 inches long / wide, 28 inches deep, (Top shelf / display level).
      2. End sections:
         1. 27 inches long / wide, 45 inches deep, 45 inches high. (Overall).
         2. 42 inches long / wide, 18 inches deep, (First shelf /display level).
         3. 36 inches long / wide, 15 inches deep, (Second shelf /display level).
         4. 28 inches long / wide, 15 inches deep, (Top shelf / display level).
      3. Chalkboard sign:
         1. 35 inches long / wide, 21 inches high.
      4. Dimensional sizes may vary plus or minus 2 inches in any direction.
   2. **Salient Characteristics that shall be provided:**
      1. Oak construction.
      2. Moisture resistant protective sealant.
      3. Display shelves to be adjustable.
      4. Each section to have a minimum of 2 removable shelves for advanced display options.
      5. Base section to have a black plastic or flexible vinyl bumper on front and back.
      6. End sections to have a minimum 1 inch wide black plastic or flexible vinyl bumper on the 3 sides facing outwards.
      7. Casters: 2 swivel and minimum 2 locking per section.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****