# Purpose of this Equipment: To transport and merchandize cartons of milk from the walk-in cooler side for patron selection.

1. **Federal Supply Class:** 7125
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 2G10-A: 39 inches long / wide, 26 inches deep, 66 inches high
      2. 2G10-B: 27 inches long / wide, 26 inches deep, 66 inches high
      3. Dimensional sizes, such as length, width, and height are allowed to vary + / - 1 inch
   2. **Salient Characteristics that shall be provided:** 
      1. 2G10-A, 120 gallon capacity
         1. 1,200 lb. capacity
         2. Four swivel castors
      2. 2G10-B, 80 gallon capacity
         1. 800 lb. capacity
         2. Two swivel, two fixed castors
      3. Five shelves
      4. Zinc Plated wired shelves
      5. Ridged or nestable frame design
      6. Stainless frame or zinc plated lacquer dip finished frame

# Industry Standards / Requirement(s): N / A

* 1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Contractor Requirements:

* + 1. Must be shipped ready to assemble and use.
    2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
       1. Point of Contact for Service.
       2. N / A
       3. N / A
    3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY:** \_\_\_\_\_\_\_

**2G10-A (120 gallon) \_\_\_\_ \_\_\_\_ 2G10-B (80 gallon)**

****