1. **Purpose of this Equipment:** To transport product for stocking shelves.
2. **Federal Supply Class**: 7320
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. 63 inches long / wide, 16 inches deep, 61 inches high.
		2. Dimensional sizes may vary no more than 1 inch in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. All welded steel construction.
		2. Powder coating.
		3. Minimum 1500-pound capacity.
		4. Anti-skid diamond plate metal deck.
		5. Four 4-inch swivel casters and two 8-inch rigid non-marking casters.
		6. Removable end push/pull handles constructed of steel tubing with cross support straps.

# Industry Standards Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_\_\_\_\_**

****