# Purpose of this Equipment: To water plants and floral displays.

1. **Federal Supply Class:** 4510
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Dimensional sizes, such as length, width, and height are not critical to this equipment.
	2. **Salient Characteristics that shall be provided:**
		1. Sealed, permanently pressurized system.
		2. Corrosion-resistant steel tank.
		3. Casters for easy mobility.
		4. Mist and spray nozzles.
		5. Side pouch or hook for tube storage.
		6. Spray wand with shut-off valve.
		7. Threaded faucet adapter.
		8. Minimum 12 foot watering hose.
		9. Minimum 12 gallon capacity.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service.
		2. Installation and Operating Instructions.
		3. Parts List.
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****