# Purpose of this Equipment: To improve customer service and eliminate waiting lines.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Dimensional sizes, such as length, width, and height are not critical to this equipment.
	2. **Salient Characteristics that shall be provided:**
		1. Electronic 3-Digit light emitting diode (LED) display with minimum 4 inch red numbers
		2. 1 ticket dispenser
		3. “Take A Number” sign
		4. 1 roll of tickets
		5. Minimum one remote control
		6. Floor or counter top stand
		7. Wireless operation

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# Standard U.S.A. electrical specifications: 120 volts, 60 Hertz, 1 phase.

# Standard Contractor Requirements:

* 1. Must be shipped ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****