1. **Purpose of this Equipment:** To store frozen and refrigerated food products for break room use.
2. **Federal Supply Class:** 4110
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. 28 inches long / wide, 30 inches deep, 60 inches high. Dimensional sizes, such as length, width, and height are not critical to this equipment so long as this equipment is an upright floor model.
	2. **Salient Characteristics that shall be provided:**
		1. Minimum 14 cubic feet storage capacity.
		2. Two door upright model with freezer section.
		3. Reversible doors.
		4. Fixed door storage.
		5. Up-front temperature controls for freezer and refrigerator sections.
		6. Interior light for refrigerated section.
		7. Crisper bins.
		8. Minimum two adjustable and removable shelves in refrigerated section.
		9. Frost-free.
		10. ADA Compliant.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: Underwriters Laboratory (UL) listed
		2. Energy Star Compliant.
		3. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
		4. After warranty period use a one- time service call with store GPC as required.
		5. Self-repair or replace the unit as required.

# Color Requirement(s): White enamel*.*

1. **Electrical Requirements:**

# Standard U.S.A. electrical specifications: 115volts, 60 Hertz, 1phase, with a maximum amperage draw of 15 amps.

# Standard Contractor Requirements:

* 1. Must be shipped ready to, make utility connections, plug in,and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****