# Purpose of this Equipment: To measure the fat content of ground beef

1. **Federal Supply Class:** 6695
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Cannot exceed 15 inches long / wide, 10 inches deep, 20 inches high
   2. **Salient Characteristics that shall be provided:**
      1. Electric heating system
      2. Gauge, scale or other means to measure fat content
      3. Indicates fat content to within 1% accuracy
      4. Carrying case

# Industry Standards / Requirement(s):

* + 1. Industry Standards: Underwriters Laboratory (UL) listed or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology Requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:**

# \_\_\_\_\_ Standard U.S.A. electrical specifications: 115 volts, 60 Hertz, 1 phase

# \_\_\_\_\_ Pacific Theater stores 115 V / 50 HZ / 1 PH (Applies to these stores only: Atsugi, Misawa, Sagami, Sagamihara, Yokosuka, Yokota, Camp Zama, and Kanto Plains CDC. All other stores are standard U.S.A. 60 cycle voltages.)

# \_\_\_\_\_ European stores 220 V / 50 HZ / 1 PH

# Cord with a NEMA Standard plug, or a manufacturer’s equivalent to comply with the equipment plug in requirements

# NOTE: the operating range for 120 volts is 110 to 120 volts; the operating range for 220 volts is 208 to 230 volts

# Standard Contractor Requirements:

* 1. Must be shipped ready to plug inand use
  2. This equipment requires disposal: place in a specified area and dispose
  3. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  4. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

