# Purpose of this Equipment: Transport grocery bags to the parking lot for customers in. Designed to accommodate both paper and plastic bags.

1. **Federal Supply Class:** 7290
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 28 inches long / wide, 22 inches deep, 44 inches high.
      2. Dimensional sizes such as length, width, and height may vary no more than 2 inches in any direction.
   2. **Salient Characteristics that shall be provided:**
      1. Frame consisting of wrap around steel tubing.
      2. Grey powder coat finish.
      3. Cart enclosed on 3 sides, upper folding shelf with hooks provided to hang plastic bags.
      4. Four non-marking, solid rubber pneumatic, self-lubricating roller bearing wheels.
      5. Front wheels to be minimum 5 inch swivel.
      6. **2E00-C:** rear wheels to be minimum 5 inch fixed.
      7. **2E00-D:** rear wheels to be minimum 10 inch fixed.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology Requirements:** N / A

# Color Requirement(s): Grey

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY:** \_\_\_\_\_ (ea.) 2E00-C (regular) \_\_\_\_\_ (ea.) 2E00-D (rough terrain)

****