# Purpose of this Equipment: To provide a 360 degree bakery goods display for patron self-service selections.

1. **Federal Supply Class:** 7310
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 78 inches long / wide, 37 inches deep, 28 inches high, (table).
      2. 36 inches long / wide, 20 inches deep, 14 inches high, (top shelf).
      3. Dimensional sizes may vary plus or minus 2 inches in any direction.
   2. **Salient Characteristics that shall be provided:**
      1. Consists of 2 separate parts, the table and the removable top shelf.
      2. Oak construction.
      3. Moisture resistant protective sealant.
      4. Table components:
         1. Side drop leaves.
         2. Casters: 2 swivel and minimum 2 locking.
         3. Plastic bumpers.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): Light Oak

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped pre-drilled and ready to assemble.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****