# Purpose of this Equipment: To store, transport or for proofing baking pans / trays.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. Rack: 21 inches long / wide, 26 inches deep, 65 inches high. Dimensional sizes may vary no more than 1 inch in any direction, so long as this equipment is capable of holding 18 inch by 26-inch trays.
      2. Cover: 23 inches long / wide, 28 inches deep, 61 inches high. Dimensional sizes may vary no more than 1 inch in any direction to this equipment in order for the cover to fit properly over the rack.
   2. **Salient Characteristics that shall be provided:**
      1. Rack:
         1. Square tubular aluminum frame with tray slides.
         2. Net storage capacity of 18 trays.
         3. Minimum 5-inch diameter swivel casters.

**3.2.2** Cover:

**3.2.2.1** Heavy duty clear plastic.

**3.2.2.2** Reinforced zippers.

# Industry Standards Requirement(s):

* + 1. Industry Standards: National Sanitation Foundation (NSF) certification, or equivalent. CE is not acceptable for a standard.
    2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.

# Color Requirement(s): N / A

1. **Electrical Requirements:**  N / A

# Contractor Requirements:

* 1. Must be shipped ready to use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_\_\_\_\_**

****