1. **Purpose of Equipment:** To stock wet produce.
2. **Federal Supply Class:** 7320
3. **Generalized Operating Specifications:**
	1. Dimensions:
		1. 43 inches long, 25 inches wide, 36 inches high.
		2. Dimensional sizes may vary no more than 1 inch in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Aluminum, galvanized steel or stainless steel.
		2. Minimum 600-pound capacity.
		3. Removable and reversible pan as the upper shelf.
		4. Non-removable solid surface lower deck.
		5. Steel handle.
		6. Two swivel and two rigid non-marking casters.

# Industry Standards / Requirement(s): N / A

* 1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

 **STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

 