1. **Purpose of this Equipment:** To transport merchandise in the warehouse and for stocking shelves.
2. **Federal Supply Class:** 7320
3. **General Operating Specifications:**
	1. **Dimensions:**
		1. 54 inches long / wide, 29.5 inches deep, 39.5 inches high.
		2. Dimensional sizes may vary no more than 1 inch in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Steel frame with steel deck
		2. Minimum 2000-pound capacity
		3. Non-marking casters
		4. Nestable

# Industry Standards / Requirement(s):

* + 1. Industry Standards: N / A
		2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Contractor Requirements:

* 1. Must be shipped ready to use
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_\_\_\_\_**

****