# Purpose of this Equipment: For break room, administrative and training use.

1. **Federal Supply Class:** 7110
2. **General Operating Specifications:**
	1. **Dimensions:**
		1. Chair: 22 inches long, 22 inches wide, 32 inches high.
		2. Dimensions such as length, width, and height may vary plus or minus 3 inches in any direction.
	2. **Salient Characteristics that shall be provided:**
		1. Chair:
			1. Steel construction.
			2. Seat and backs contoured.
			3. Sled base design for stability.
			4. Stackable.
			5. Floor glides to protect floor surface.
			6. Armless.
			7. Minimum 300 pound capacity.
		2. Dolly:
			1. Minimum four caster wheels.
			2. Minimum chair capacity of 30 high.

# Industry Standards / Requirement(s):

* + 1. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
	1. **Information Technology requirements:** N / A

# Color Requirement(s):

* + 1. Frame for chairs: Black or chrome.
		2. Chair: Black or Burgundy.
1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to assemble and use.
	2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
		1. Point of Contact for Service
		2. Installation and Operating Instructions
		3. Parts List
	3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_** (1) carton = (4) chairs \_\_\_\_\_\_\_ each (dolly)

****